Company Name:  
	Your Website:
Phone #: 
Your Email:	Sing Square Log Homes, Inc.
DBA: Sing Core
PO Box 1691, McCleary, WA 98557
info@singhome.com
O: 360-495-3577/F: 360-495-4585
Quote Request Form	
Contact Person:			
Delivery Address:  		
When do you need order by?	What is the application for this product?	What is your estimated budget for this product?

Range to:_____________  From:_____________	
Panels may require to be acclimated to your area especially for over-length or thin panels.  Certain storage guidelines should be followed.  Call for details
*We guarantee our panels for flatness within the AWI standards or we will build you replacement panels without any extra cost to you.
Quantity of Panels	Length in Inches	Width in Inches	Core Skin in Thickness	Total Thickness in
Inches	Solid Edge or Open Edge 	
Special Instructions/Panel Quality	Panel Quality
(Check One)	
			TOP						Standard
Paint Grade	
			BOTTOM						Upgrades	
			TOP						Standard 
Paint Grade	
			BOTTOM						Upgrades	
			TOP						Standard 
Paint Grade	
			BOTTOM						Upgrades	
Upgrade Choices  (all upgrades will increase price of panels)  (*Standard Panels come w/ luan or birch skins and cedar or fir solid wood edging)	
SKINS
If “other” please specify	GRID SIZES
(Grids larger than 2” could show under thinner skins)	HARDWOOD 
SOLID WOOD EDGING	WINDOW 
CUT-OUTS	
	Plywood			MDF			Aluminum			Steel		OTHER		Smaller
2” or less	x	3”x 3”
Standard		Larger
4” or more		POPLAR		MAPLE		
STANDARD EXAMPLE BELOW                                                          STANDARD EXAMPLE BELOW                                              STANDARD EXAMPLE BELOW           	

1	
95”	
47”	TOP	¼” Luan	1-1/2”	1-1/4”	N/A	X	Standard Paint Grade	
			BOTTOM	¼” Luan					Custom
	
IMPORTANT! ALL PANELS COME AS PAINT GRADE - NOT – PAINT READY!   CUSTOMER IS RESPONSIBLE TO GET PRODUCT TO FINISHED 
QUALITY. SING CORE IS NOT RESPONSIBLE FOR AMOUNT OF TIME or EFFORT NEEDED TO GET PRODUCT TO DESIRED FINISHED QUALITY!

SIGNATURE:		DATE: